Line Level Notes

Andrew Schroeder | 2019-02-18

Output level from instruments:

A VU meter configured for professional line level reads 0dB when the input has , meaning that a reading of +4dB will be shown when a sin wave of is present, the maximum undistorted level.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| 0 | 3.53 | 1.77 | 1.25 | 1.125 | 1.77 |
| +4 | 5.66 | 2.83 | 2 | 1.80 | **2.83** |